主页 » 其它
# MSSQL Server - Surface Area Configuration Carry out the procedure given below to enable the option Using both TCP/IP and named pipes in Remote Connections. This configuration is applicable for SQL Server 2005 & above. In the SQL Server 2005 Surface Area Configuration configuration screen, select MSSQLSERVER > Database Engine > Remote Connections component on the left side of the configuration screen. Select the Local and remote connections > Using both TCP/IP and named pipes option on the right side of the screen. Refer the screen shot given below.

版权所有 © 2015, 卓豪（北京）技术有限公司， 保留一切权利